yiuchunkit_1230@yahoo.com.hk
SatRef GNSS Automatic Computation Service - Acknowledgement
The following files are received on 2013-06-05 18:46:00

1. Nail1560.13n       12 Kb
2. Nail1560.13o      201 Kb
3. Nail1561.13n       12 Kb
4. Nail1561.13o      190 Kb

Selected Options:
Computation Accuracy              = 10mm+3ppm
Maximum Sigma                     = 30mm
Reference Station                 = HKSS,HKFN,HKKT
Minimum No. of Reference Station  = 2
Minimum No. of Session            = 2
Minimum Duration                  = 15 min.
Minimum Interval                  = 30 min.
Minimum No. of Baseline           = 3
Maximum GDOP                      = 5.0
Epoch Rate                        = 5 sec.
Divide Observation file for every = N.A.
Land Boundary Survey Standard     = True
Check Origin                      = True
Reject Large GDOP                 = True
Elevation Mask                    = 15 deg.

The data will be processed and the result will be sent to you shortly.

Thank you for choosing SatRef GNSS Automatic Computation Service.



Geodetic Survey Section
Survey and Mapping Office
Lands Department
..
