chantai-man@hotmail.com
SatRef GNSS Automatic Computation Service - Acknowledgement
The following files are received on 2012-06-28 07:56:00

1. KL2_AM0-1.12o      917 Kb
2. KL2_AM0-2.12o      833 Kb

Selected Options:
Reference Station                 = Nearest 3
Computation Accuracy              = 10mm+3ppm
Minimum No. of Reference Station  = 2
Minimum No. of Session            = 2
Minimum Duration                  = 15 min.
Minimum Interval                  = 30 min.
Minimum No. of Baseline           = 3
Maximum GDOP                      = 5.0
Epoch Rate                        = 5 sec.
Divide Observation file for every = N.A.
Land Boundary Survey Standard     = True
Check Origin                      = True
Reject Large GDOP                 = True
Elevation Mask                    = 15 deg.

The data will be processed and the result will be sent to you shortly.

Thank you for choosing SatRef GNSS Automatic Computation Service.



Geodetic Survey Section
Survey and Mapping Office
Lands Department
